IRremoteESP8266: Hitachi424Protocol Union Reference

IRremoteESP8266

Public Attributes | List of all members
Hitachi424Protocol Union Reference

Native representation of a Hitachi 53-byte/424-bit A/C message. More...

`#include <ir_Hitachi.h>`

## Public Attributes

uint8_t | raw [kHitachiAc424StateLength]
| The state in native code. More...
struct {
uint8_t pad0 [11]
uint8_t Button:8
uint8_t __pad0__:8
uint8_t __pad1__:2
uint8_t Temp:6
uint8_t pad1 [11]
uint8_t Mode:4
uint8_t Fan:4
uint8_t __pad2__:8
uint8_t Power:8
uint8_t pad2 [7]
uint8_t SwingH:3
uint8_t __pad3__:5
uint8_t __pad4__:8
uint8_t __pad5__:5
uint8_t SwingV:1
uint8_t __pad6__:2
}; |

## Detailed Description

Native representation of a Hitachi 53-byte/424-bit A/C message.

## Member Data Documentation

## ◆ @45

struct { ... }

## ◆ __pad0__

uint8_t Hitachi424Protocol::__pad0__

## ◆ __pad1__

uint8_t Hitachi424Protocol::__pad1__

## ◆ __pad2__

uint8_t Hitachi424Protocol::__pad2__

## ◆ __pad3__

uint8_t Hitachi424Protocol::__pad3__

## ◆ __pad4__

uint8_t Hitachi424Protocol::__pad4__

## ◆ __pad5__

uint8_t Hitachi424Protocol::__pad5__

## ◆ __pad6__

uint8_t Hitachi424Protocol::__pad6__

## ◆ Button

uint8_t Hitachi424Protocol::Button

## ◆ Fan

uint8_t Hitachi424Protocol::Fan

## ◆ Mode

uint8_t Hitachi424Protocol::Mode

## ◆ pad0

uint8_t Hitachi424Protocol::pad0[11]

## ◆ pad1

uint8_t Hitachi424Protocol::pad1[11]

## ◆ pad2

uint8_t Hitachi424Protocol::pad2[7]

## ◆ Power

uint8_t Hitachi424Protocol::Power

## ◆ raw

uint8_t Hitachi424Protocol::raw[kHitachiAc424StateLength]

The state in native code.

## ◆ SwingH

uint8_t Hitachi424Protocol::SwingH

## ◆ SwingV

uint8_t Hitachi424Protocol::SwingV

## ◆ Temp

uint8_t Hitachi424Protocol::Temp

The documentation for this union was generated from the following file:

- src/ir_Hitachi.h