IRremoteESP8266: CarrierProtocol Union Reference

IRremoteESP8266

Public Attributes | List of all members
CarrierProtocol Union Reference

Native representation of a Carrier A/C message. More...

`#include <ir_Carrier.h>`

## Public Attributes

uint64_t | raw
| The state of the IR remote. More...
struct {
uint8_t __pad0__:8
uint8_t __pad1__:8
uint8_t Sum:4
uint8_t Mode:2
uint8_t Fan:2
uint8_t Temp:4
uint8_t __pad2__:1
uint8_t SwingV:1
uint8_t __pad3__:2
uint8_t __pad4__:4
uint8_t Power:1
uint8_t OffTimerEnable:1
uint8_t OnTimerEnable:1
uint8_t Sleep:1
uint8_t __pad5__:8
uint8_t __pad6__:4
uint8_t OnTimer:4
uint8_t __pad7__:4
uint8_t OffTimer:4
}; |

## Detailed Description

Native representation of a Carrier A/C message.

## Member Data Documentation

## ◆ @7

struct { ... }

## ◆ __pad0__

uint8_t CarrierProtocol::__pad0__

## ◆ __pad1__

uint8_t CarrierProtocol::__pad1__

## ◆ __pad2__

uint8_t CarrierProtocol::__pad2__

## ◆ __pad3__

uint8_t CarrierProtocol::__pad3__

## ◆ __pad4__

uint8_t CarrierProtocol::__pad4__

## ◆ __pad5__

uint8_t CarrierProtocol::__pad5__

## ◆ __pad6__

uint8_t CarrierProtocol::__pad6__

## ◆ __pad7__

uint8_t CarrierProtocol::__pad7__

## ◆ Fan

uint8_t CarrierProtocol::Fan

## ◆ Mode

uint8_t CarrierProtocol::Mode

## ◆ OffTimer

uint8_t CarrierProtocol::OffTimer

## ◆ OffTimerEnable

uint8_t CarrierProtocol::OffTimerEnable

## ◆ OnTimer

uint8_t CarrierProtocol::OnTimer

## ◆ OnTimerEnable

uint8_t CarrierProtocol::OnTimerEnable

## ◆ Power

uint8_t CarrierProtocol::Power

## ◆ raw

uint64_t CarrierProtocol::raw

The state of the IR remote.

## ◆ Sleep

uint8_t CarrierProtocol::Sleep

## ◆ Sum

uint8_t CarrierProtocol::Sum

## ◆ SwingV

uint8_t CarrierProtocol::SwingV

## ◆ Temp

uint8_t CarrierProtocol::Temp

The documentation for this union was generated from the following file:

- src/ir_Carrier.h