IRremoteESP8266: PanasonicAc32Protocol Union Reference

IRremoteESP8266

Public Attributes | List of all members
PanasonicAc32Protocol Union Reference

Native representation of a Panasonic 32-bit A/C message. More...

`#include <ir_Panasonic.h>`

## Public Attributes

uint32_t | raw
| The state in IR code form. More...
struct {
uint8_t __pad0__:3
uint8_t SwingH:1
uint8_t SwingV:3
uint8_t __pad1__:1
| Always appears to be set. (1) More...
uint8_t __pad2__:8
uint8_t Temp:4
uint8_t Fan:4
uint8_t Mode:3
uint8_t PowerToggle:1
uint8_t __pad3__:4
}; |

## Detailed Description

Native representation of a Panasonic 32-bit A/C message.

## Member Data Documentation

## ◆ @68

struct { ... }

## ◆ __pad0__

uint8_t PanasonicAc32Protocol::__pad0__

## ◆ __pad1__

uint8_t PanasonicAc32Protocol::__pad1__

Always appears to be set. (1)

## ◆ __pad2__

uint8_t PanasonicAc32Protocol::__pad2__

## ◆ __pad3__

uint8_t PanasonicAc32Protocol::__pad3__

## ◆ Fan

uint8_t PanasonicAc32Protocol::Fan

## ◆ Mode

uint8_t PanasonicAc32Protocol::Mode

## ◆ PowerToggle

uint8_t PanasonicAc32Protocol::PowerToggle

## ◆ raw

uint32_t PanasonicAc32Protocol::raw

The state in IR code form.

## ◆ SwingH

uint8_t PanasonicAc32Protocol::SwingH

## ◆ SwingV

uint8_t PanasonicAc32Protocol::SwingV

## ◆ Temp

uint8_t PanasonicAc32Protocol::Temp

The documentation for this union was generated from the following file:

- src/ir_Panasonic.h