IRremoteESP8266: Todo List

IRremoteESP8266

Todo List

Member IRrecv::decodeLasertag (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kLasertagBits, const bool strict=true)
  Convert to using `matchManchester()` if we can.
Member IRrecv::decodeRC5 (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kRC5XBits, const bool strict=true)
  Serious testing of the RC-5X and strict aspects needs to be done.
Member IRrecv::decodeRC6 (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kRC6Mode0Bits, const bool strict=false)
  Testing of the strict compliance aspects.
Member IRrecv::decodeSharp (decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kSharpBits, const bool strict=true, const bool expansion=true)
  Need to ensure capture of the inverted message as it can be missed due to the interrupt timeout used to detect an end of message. Several compliance checks are disabled until that is resolved.
Member IRrecv::matchManchesterData (volatile const uint16_t *data_ptr, uint64_t *result_ptr, const uint16_t remaining, const uint16_t nbits, const uint16_t half_period, const uint16_t starting_balance=0, const uint8_t tolerance=kUseDefTol, const int16_t excess=kMarkExcess, const bool MSBfirst=true, const bool GEThomas=true)
  Clean up and optimise this. It is just "get it working code" atm.
Member IRSamsungAc::getSwing (void) const
  (Hollako) Explain why sometimes the LSB of remote_state[9] is a 1. e.g. 0xAE or 0XAF for swing move.
Member IRSamsungAc::setSwing (const bool on)
  (Hollako) Explain why sometimes the LSB of remote_state[9] is a 1. e.g. 0xAE or 0XAF for swing move.
Member IRsend::sendLasertag (uint64_t data, uint16_t nbits=kLasertagBits, uint16_t repeat=kLasertagMinRepeat)
  Convert this to use `sendManchester()` if we can.`
Member IRsend::sendRC5 (const uint64_t data, uint16_t nbits=kRC5XBits, const uint16_t repeat=kNoRepeat)
  Testing of the RC-5X components.
Member IRsend::sendSAMSUNG (const uint64_t data, const uint16_t nbits=kSamsungBits, const uint16_t repeat=kNoRepeat)
  Confirm that is actually how Samsung sends a repeat. The refdoc doesn't indicate it is true.
Member MideaProtocol::__pad2__
  Find out what this bit controls.