IRremoteESP8266: Member List

IRremoteESP8266

IRKelvinatorAC Member List

This is the complete list of members for IRKelvinatorAC, including all inherited members.

_ | IRKelvinatorAC | private
_irsend | IRKelvinatorAC | private
begin(void) | IRKelvinatorAC |
calcBlockChecksum(const uint8_t *block, const uint16_t length=kKelvinatorStateLength/2) | IRKelvinatorAC | static
calibrate(void) | IRKelvinatorAC | inline
checksum(void) | IRKelvinatorAC | private
convertMode(const stdAc::opmode_t mode) | IRKelvinatorAC | static
fixup(void) | IRKelvinatorAC | private
getFan(void) const | IRKelvinatorAC |
getIonFilter(void) const | IRKelvinatorAC |
getLight(void) const | IRKelvinatorAC |
getMode(void) const | IRKelvinatorAC |
getPower(void) const | IRKelvinatorAC |
getQuiet(void) const | IRKelvinatorAC |
getRaw(void) | IRKelvinatorAC |
getSwingHorizontal(void) const | IRKelvinatorAC |
getSwingVertical(void) const | IRKelvinatorAC |
getTemp(void) const | IRKelvinatorAC |
getTurbo(void) const | IRKelvinatorAC |
getXFan(void) const | IRKelvinatorAC |
IRKelvinatorAC(const uint16_t pin, const bool inverted=false, const bool use_modulation=true) | IRKelvinatorAC | explicit
off(void) | IRKelvinatorAC |
on(void) | IRKelvinatorAC |
send(const uint16_t repeat=kKelvinatorDefaultRepeat) | IRKelvinatorAC |
setFan(const uint8_t speed) | IRKelvinatorAC |
setIonFilter(const bool on) | IRKelvinatorAC |
setLight(const bool on) | IRKelvinatorAC |
setMode(const uint8_t mode) | IRKelvinatorAC |
setPower(const bool on) | IRKelvinatorAC |
setQuiet(const bool on) | IRKelvinatorAC |
setRaw(const uint8_t new_code[]) | IRKelvinatorAC |
setSwingHorizontal(const bool on) | IRKelvinatorAC |
setSwingVertical(const bool on) | IRKelvinatorAC |
setTemp(const uint8_t degrees) | IRKelvinatorAC |
setTurbo(const bool on) | IRKelvinatorAC |
setXFan(const bool on) | IRKelvinatorAC |
stateReset(void) | IRKelvinatorAC |
toCommon(void) const | IRKelvinatorAC |
toCommonFanSpeed(const uint8_t speed) | IRKelvinatorAC | static
toCommonMode(const uint8_t mode) | IRKelvinatorAC | static
toString(void) const | IRKelvinatorAC |
validChecksum(const uint8_t state[], const uint16_t length=kKelvinatorStateLength) | IRKelvinatorAC | static