IRremoteESP8266: Member List

IRremoteESP8266

IRsend Member List

This is the complete list of members for IRsend, including all inherited members.

_delayMicroseconds(uint32_t usec) | IRsend |
_dutycycle | IRsend | private
_freq_unittest | IRsend | private
_sendSony(const uint64_t data, const uint16_t nbits, const uint16_t repeat, const uint16_t freq) | IRsend | private
begin() | IRsend |
calcUSecPeriod(uint32_t hz, bool use_offset=true) | IRsend | private
calibrate(uint16_t hz=38000U) | IRsend |
defaultBits(const decode_type_t protocol) | IRsend | static
enableIROut(uint32_t freq, uint8_t duty=kDutyDefault) | IRsend |
encodeDoshisha(const uint8_t command, const uint8_t channel=0) | IRsend |
encodeJVC(uint8_t address, uint8_t command) | IRsend |
encodeLG(uint16_t address, uint16_t command) | IRsend |
encodeMagiQuest(const uint32_t wand_id, const uint16_t magnitude) | IRsend |
encodeMetz(const uint8_t address, const uint8_t command, const bool toggle=false) | IRsend | static
encodeNEC(uint16_t address, uint16_t command) | IRsend |
encodePanasonic(const uint16_t manufacturer, const uint8_t device, const uint8_t subdevice, const uint8_t function) | IRsend |
encodePioneer(uint16_t address, uint16_t command) | IRsend |
encodeRC5(const uint8_t address, const uint8_t command, const bool key_released=false) | IRsend |
encodeRC5X(const uint8_t address, const uint8_t command, const bool key_released=false) | IRsend |
encodeRC6(const uint32_t address, const uint8_t command, const uint16_t mode=kRC6Mode0Bits) | IRsend |
encodeSAMSUNG(const uint8_t customer, const uint8_t command) | IRsend |
encodeSanyoLC7461(uint16_t address, uint8_t command) | IRsend |
encodeSharp(const uint16_t address, const uint16_t command, const uint16_t expansion=1, const uint16_t check=0, const bool MSBfirst=false) | IRsend |
encodeSony(const uint16_t nbits, const uint16_t command, const uint16_t address, const uint16_t extended=0) | IRsend |
IRpin | IRsend | private
IRsend(uint16_t IRsendPin, bool inverted=false, bool use_modulation=true) | IRsend | explicit
ledOff() | IRsend | protected
ledOn() | IRsend | protected
mark(uint16_t usec) | IRsend |
minRepeats(const decode_type_t protocol) | IRsend | static
modulation | IRsend | private
offTimePeriod | IRsend | private
onTimePeriod | IRsend | private
outputOff | IRsend | protected
outputOn | IRsend | protected
periodOffset | IRsend | private
send(const decode_type_t type, const uint64_t data, const uint16_t nbits, const uint16_t repeat=kNoRepeat) | IRsend |
send(const decode_type_t type, const uint8_t *state, const uint16_t nbytes) | IRsend |
sendAirwell(uint64_t data, uint16_t nbits=kAirwellBits, uint16_t repeat=kAirwellMinRepeats) | IRsend |
sendAiwaRCT501(uint64_t data, uint16_t nbits=kAiwaRcT501Bits, uint16_t repeat=kAiwaRcT501MinRepeats) | IRsend |
sendAmcor(const unsigned char data[], const uint16_t nbytes=kAmcorStateLength, const uint16_t repeat=kAmcorDefaultRepeat) | IRsend |
sendArgo(const unsigned char data[], const uint16_t nbytes=kArgoStateLength, const uint16_t repeat=kArgoDefaultRepeat) | IRsend |
sendCarrierAC(uint64_t data, uint16_t nbits=kCarrierAcBits, uint16_t repeat=kCarrierAcMinRepeat) | IRsend |
sendCarrierAC40(uint64_t data, uint16_t nbits=kCarrierAc40Bits, uint16_t repeat=kCarrierAc40MinRepeat) | IRsend |
sendCarrierAC64(uint64_t data, uint16_t nbits=kCarrierAc64Bits, uint16_t repeat=kCarrierAc64MinRepeat) | IRsend |
sendCOOLIX(uint64_t data, uint16_t nbits=kCoolixBits, uint16_t repeat=kCoolixDefaultRepeat) | IRsend |
sendCoronaAc(const uint8_t data[], const uint16_t nbytes=kCoronaAcStateLength, const uint16_t repeat=kNoRepeat) | IRsend |
sendDaikin(const unsigned char data[], const uint16_t nbytes=kDaikinStateLength, const uint16_t repeat=kDaikinDefaultRepeat) | IRsend |
sendDaikin128(const unsigned char data[], const uint16_t nbytes=kDaikin128StateLength, const uint16_t repeat=kDaikin128DefaultRepeat) | IRsend |
sendDaikin152(const unsigned char data[], const uint16_t nbytes=kDaikin152StateLength, const uint16_t repeat=kDaikin152DefaultRepeat) | IRsend |
sendDaikin160(const unsigned char data[], const uint16_t nbytes=kDaikin160StateLength, const uint16_t repeat=kDaikin160DefaultRepeat) | IRsend |
sendDaikin176(const unsigned char data[], const uint16_t nbytes=kDaikin176StateLength, const uint16_t repeat=kDaikin176DefaultRepeat) | IRsend |
sendDaikin2(const unsigned char data[], const uint16_t nbytes=kDaikin2StateLength, const uint16_t repeat=kDaikin2DefaultRepeat) | IRsend |
sendDaikin216(const unsigned char data[], const uint16_t nbytes=kDaikin216StateLength, const uint16_t repeat=kDaikin216DefaultRepeat) | IRsend |
sendDaikin64(const uint64_t data, const uint16_t nbits=kDaikin64Bits, const uint16_t repeat=kDaikin64DefaultRepeat) | IRsend |
sendData(uint16_t onemark, uint32_t onespace, uint16_t zeromark, uint32_t zerospace, uint64_t data, uint16_t nbits, bool MSBfirst=true) | IRsend |
sendDelonghiAc(uint64_t data, uint16_t nbits=kDelonghiAcBits, uint16_t repeat=kDelonghiAcDefaultRepeat) | IRsend |
sendDenon(uint64_t data, uint16_t nbits=kDenonBits, uint16_t repeat=kNoRepeat) | IRsend |
sendDISH(uint64_t data, uint16_t nbits=kDishBits, uint16_t repeat=kDishMinRepeat) | IRsend |
sendDoshisha(const uint64_t data, uint16_t nbits=kDoshishaBits, const uint16_t repeat=kNoRepeat) | IRsend |
sendEcoclim(const uint64_t data, const uint16_t nbits=kEcoclimBits, const uint16_t repeat=kNoRepeat) | IRsend |
sendElectraAC(const unsigned char data[], const uint16_t nbytes=kElectraAcStateLength, const uint16_t repeat=kNoRepeat) | IRsend |
sendElitescreens(const uint64_t data, const uint16_t nbits=kEliteScreensBits, const uint16_t repeat=kEliteScreensDefaultRepeat) | IRsend |
sendEpson(uint64_t data, uint16_t nbits=kEpsonBits, uint16_t repeat=kEpsonMinRepeat) | IRsend |
sendFujitsuAC(const unsigned char data[], const uint16_t nbytes, const uint16_t repeat=kFujitsuAcMinRepeat) | IRsend |
sendGC(uint16_t buf[], uint16_t len) | IRsend |
sendGeneric(const uint16_t headermark, const uint32_t headerspace, const uint16_t onemark, const uint32_t onespace, const uint16_t zeromark, const uint32_t zerospace, const uint16_t footermark, const uint32_t gap, const uint64_t data, const uint16_t nbits, const uint16_t frequency, const bool MSBfirst, const uint16_t repeat, const uint8_t dutycycle) | IRsend |
sendGeneric(const uint16_t headermark, const uint32_t headerspace, const uint16_t onemark, const uint32_t onespace, const uint16_t zeromark, const uint32_t zerospace, const uint16_t footermark, const uint32_t gap, const uint32_t mesgtime, const uint64_t data, const uint16_t nbits, const uint16_t frequency, const bool MSBfirst, const uint16_t repeat, const uint8_t dutycycle) | IRsend |
sendGeneric(const uint16_t headermark, const uint32_t headerspace, const uint16_t onemark, const uint32_t onespace, const uint16_t zeromark, const uint32_t zerospace, const uint16_t footermark, const uint32_t gap, const uint8_t *dataptr, const uint16_t nbytes, const uint16_t frequency, const bool MSBfirst, const uint16_t repeat, const uint8_t dutycycle) | IRsend |
sendGICable(uint64_t data, uint16_t nbits=kGicableBits, uint16_t repeat=kGicableMinRepeat) | IRsend |
sendGoodweather(const uint64_t data, const uint16_t nbits=kGoodweatherBits, const uint16_t repeat=kGoodweatherMinRepeat) | IRsend |
sendGree(const uint64_t data, const uint16_t nbits=kGreeBits, const uint16_t repeat=kGreeDefaultRepeat) | IRsend |
sendGree(const uint8_t data[], const uint16_t nbytes=kGreeStateLength, const uint16_t repeat=kGreeDefaultRepeat) | IRsend |
sendHaierAC(const unsigned char data[], const uint16_t nbytes=kHaierACStateLength, const uint16_t repeat=kHaierAcDefaultRepeat) | IRsend |
sendHaierACYRW02(const unsigned char data[], const uint16_t nbytes=kHaierACYRW02StateLength, const uint16_t repeat=kHaierAcYrw02DefaultRepeat) | IRsend |
sendHitachiAC(const unsigned char data[], const uint16_t nbytes=kHitachiAcStateLength, const uint16_t repeat=kHitachiAcDefaultRepeat) | IRsend |
sendHitachiAC1(const unsigned char data[], const uint16_t nbytes=kHitachiAc1StateLength, const uint16_t repeat=kHitachiAcDefaultRepeat) | IRsend |
sendHitachiAC2(const unsigned char data[], const uint16_t nbytes=kHitachiAc2StateLength, const uint16_t repeat=kHitachiAcDefaultRepeat) | IRsend |
sendHitachiAc3(const unsigned char data[], const uint16_t nbytes, const uint16_t repeat=kHitachiAcDefaultRepeat) | IRsend |
sendHitachiAc344(const unsigned char data[], const uint16_t nbytes=kHitachiAc344StateLength, const uint16_t repeat=kHitachiAcDefaultRepeat) | IRsend |
sendHitachiAc424(const unsigned char data[], const uint16_t nbytes=kHitachiAc424StateLength, const uint16_t repeat=kHitachiAcDefaultRepeat) | IRsend |
sendInax(const uint64_t data, const uint16_t nbits=kInaxBits, const uint16_t repeat=kInaxMinRepeat) | IRsend |
sendJVC(uint64_t data, uint16_t nbits=kJvcBits, uint16_t repeat=kNoRepeat) | IRsend |
sendKelvinator(const unsigned char data[], const uint16_t nbytes=kKelvinatorStateLength, const uint16_t repeat=kKelvinatorDefaultRepeat) | IRsend |
sendLasertag(uint64_t data, uint16_t nbits=kLasertagBits, uint16_t repeat=kLasertagMinRepeat) | IRsend |
sendLegoPf(const uint64_t data, const uint16_t nbits=kLegoPfBits, const uint16_t repeat=kLegoPfMinRepeat) | IRsend |
sendLG(uint64_t data, uint16_t nbits=kLgBits, uint16_t repeat=kNoRepeat) | IRsend |
sendLG2(uint64_t data, uint16_t nbits=kLgBits, uint16_t repeat=kNoRepeat) | IRsend |
sendLutron(uint64_t data, uint16_t nbits=kLutronBits, uint16_t repeat=kNoRepeat) | IRsend |
sendMagiQuest(const uint64_t data, const uint16_t nbits=kMagiquestBits, const uint16_t repeat=kNoRepeat) | IRsend |
sendManchester(const uint16_t headermark, const uint32_t headerspace, const uint16_t half_period, const uint16_t footermark, const uint32_t gap, const uint64_t data, const uint16_t nbits, const uint16_t frequency=38, const bool MSBfirst=true, const uint16_t repeat=kNoRepeat, const uint8_t dutycycle=kDutyDefault, const bool GEThomas=true) | IRsend |
sendManchesterData(const uint16_t half_period, const uint64_t data, const uint16_t nbits, const bool MSBfirst=true, const bool GEThomas=true) | IRsend |
sendMetz(const uint64_t data, const uint16_t nbits=kMetzBits, const uint16_t repeat=kMetzMinRepeat) | IRsend |
sendMidea(uint64_t data, uint16_t nbits=kMideaBits, uint16_t repeat=kMideaMinRepeat) | IRsend |
sendMidea24(const uint64_t data, const uint16_t nbits=kMidea24Bits, const uint16_t repeat=kMidea24MinRepeat) | IRsend |
sendMilestag2(const uint64_t data, const uint16_t nbits=kMilesTag2ShotBits, const uint16_t repeat=kMilesMinRepeat) | IRsend |
sendMirage(const unsigned char data[], const uint16_t nbytes=kMirageStateLength, const uint16_t repeat=kMirageMinRepeat) | IRsend |
sendMitsubishi(uint64_t data, uint16_t nbits=kMitsubishiBits, uint16_t repeat=kMitsubishiMinRepeat) | IRsend |
sendMitsubishi112(const unsigned char data[], const uint16_t nbytes=kMitsubishi112StateLength, const uint16_t repeat=kMitsubishi112MinRepeat) | IRsend |
sendMitsubishi136(const unsigned char data[], const uint16_t nbytes=kMitsubishi136StateLength, const uint16_t repeat=kMitsubishi136MinRepeat) | IRsend |
sendMitsubishi2(uint64_t data, uint16_t nbits=kMitsubishiBits, uint16_t repeat=kMitsubishiMinRepeat) | IRsend |
sendMitsubishiAC(const unsigned char data[], const uint16_t nbytes=kMitsubishiACStateLength, const uint16_t repeat=kMitsubishiACMinRepeat) | IRsend |
sendMitsubishiHeavy152(const unsigned char data[], const uint16_t nbytes=kMitsubishiHeavy152StateLength, const uint16_t repeat=kMitsubishiHeavy152MinRepeat) | IRsend |
sendMitsubishiHeavy88(const unsigned char data[], const uint16_t nbytes=kMitsubishiHeavy88StateLength, const uint16_t repeat=kMitsubishiHeavy88MinRepeat) | IRsend |
sendMultibrackets(const uint64_t data, const uint16_t nbits=kMultibracketsBits, const uint16_t repeat=kMultibracketsDefaultRepeat) | IRsend |
sendMWM(const unsigned char data[], const uint16_t nbytes, const uint16_t repeat=kNoRepeat) | IRsend |
sendNEC(uint64_t data, uint16_t nbits=kNECBits, uint16_t repeat=kNoRepeat) | IRsend |
sendNeoclima(const unsigned char data[], const uint16_t nbytes=kNeoclimaStateLength, const uint16_t repeat=kNeoclimaMinRepeat) | IRsend |
sendNikai(uint64_t data, uint16_t nbits=kNikaiBits, uint16_t repeat=kNoRepeat) | IRsend |
sendPanasonic(const uint16_t address, const uint32_t data, const uint16_t nbits=kPanasonicBits, const uint16_t repeat=kNoRepeat) | IRsend |
sendPanasonic64(const uint64_t data, const uint16_t nbits=kPanasonicBits, const uint16_t repeat=kNoRepeat) | IRsend |
sendPanasonicAC(const unsigned char data[], const uint16_t nbytes=kPanasonicAcStateLength, const uint16_t repeat=kPanasonicAcDefaultRepeat) | IRsend |
sendPanasonicAC32(const uint64_t data, const uint16_t nbits=kPanasonicAc32Bits, const uint16_t repeat=kPanasonicAcDefaultRepeat) | IRsend |
sendPioneer(const uint64_t data, const uint16_t nbits=kPioneerBits, const uint16_t repeat=kNoRepeat) | IRsend |
sendPronto(uint16_t data[], uint16_t len, uint16_t repeat=kNoRepeat) | IRsend |
sendRaw(const uint16_t buf[], const uint16_t len, const uint16_t hz) | IRsend |
sendRC5(const uint64_t data, uint16_t nbits=kRC5XBits, const uint16_t repeat=kNoRepeat) | IRsend |
sendRC6(const uint64_t data, const uint16_t nbits=kRC6Mode0Bits, const uint16_t repeat=kNoRepeat) | IRsend |
sendRCMM(uint64_t data, uint16_t nbits=kRCMMBits, uint16_t repeat=kNoRepeat) | IRsend |
sendSAMSUNG(const uint64_t data, const uint16_t nbits=kSamsungBits, const uint16_t repeat=kNoRepeat) | IRsend |
sendSamsung36(const uint64_t data, const uint16_t nbits=kSamsung36Bits, const uint16_t repeat=kNoRepeat) | IRsend |
sendSamsungAC(const unsigned char data[], const uint16_t nbytes=kSamsungAcStateLength, const uint16_t repeat=kSamsungAcDefaultRepeat) | IRsend |
sendSanyoAc(const uint8_t *data, const uint16_t nbytes=kSanyoAcStateLength, const uint16_t repeat=kNoRepeat) | IRsend |
sendSanyoLC7461(const uint64_t data, const uint16_t nbits=kSanyoLC7461Bits, const uint16_t repeat=kNoRepeat) | IRsend |
sendSharp(const uint16_t address, const uint16_t command, const uint16_t nbits=kSharpBits, const uint16_t repeat=kNoRepeat) | IRsend |
sendSharpAc(const unsigned char data[], const uint16_t nbytes=kSharpAcStateLength, const uint16_t repeat=kSharpAcDefaultRepeat) | IRsend |
sendSharpRaw(const uint64_t data, const uint16_t nbits=kSharpBits, const uint16_t repeat=kNoRepeat) | IRsend |
sendSherwood(uint64_t data, uint16_t nbits=kSherwoodBits, uint16_t repeat=kSherwoodMinRepeat) | IRsend |
sendSony(const uint64_t data, const uint16_t nbits=kSony20Bits, const uint16_t repeat=kSonyMinRepeat) | IRsend |
sendSony38(const uint64_t data, const uint16_t nbits=kSony20Bits, const uint16_t repeat=kSonyMinRepeat+1) | IRsend |
sendSymphony(uint64_t data, uint16_t nbits=kSymphonyBits, uint16_t repeat=kSymphonyDefaultRepeat) | IRsend |
sendTcl112Ac(const unsigned char data[], const uint16_t nbytes=kTcl112AcStateLength, const uint16_t repeat=kTcl112AcDefaultRepeat) | IRsend |
sendTechnibelAc(uint64_t data, uint16_t nbits=kTechnibelAcBits, uint16_t repeat=kTechnibelAcDefaultRepeat) | IRsend |
sendTeco(const uint64_t data, const uint16_t nbits=kTecoBits, const uint16_t repeat=kNoRepeat) | IRsend |
sendToshibaAC(const uint8_t data[], const uint16_t nbytes=kToshibaACStateLength, const uint16_t repeat=kToshibaACMinRepeat) | IRsend |
sendTranscold(const uint64_t data, const uint16_t nbits=kTranscoldBits, const uint16_t repeat=kTranscoldDefaultRepeat) | IRsend |
sendTrotec(const unsigned char data[], const uint16_t nbytes=kTrotecStateLength, const uint16_t repeat=kTrotecDefaultRepeat) | IRsend |
sendVestelAc(const uint64_t data, const uint16_t nbits=kVestelAcBits, const uint16_t repeat=kNoRepeat) | IRsend |
sendVoltas(const unsigned char data[], const uint16_t nbytes=kVoltasStateLength, const uint16_t repeat=kNoRepeat) | IRsend |
sendWhirlpoolAC(const unsigned char data[], const uint16_t nbytes=kWhirlpoolAcStateLength, const uint16_t repeat=kWhirlpoolAcDefaultRepeat) | IRsend |
sendWhynter(const uint64_t data, const uint16_t nbits=kWhynterBits, const uint16_t repeat=kNoRepeat) | IRsend |
sendZepeal(const uint64_t data, const uint16_t nbits=kZepealBits, const uint16_t repeat=kZepealMinRepeat) | IRsend |
space(uint32_t usec) | IRsend |
toggleRC5(const uint64_t data) | IRsend |
toggleRC6(const uint64_t data, const uint16_t nbits=kRC6Mode0Bits) | IRsend |