IRremoteESP8266: stdAc::state_t Struct Reference

IRremoteESP8266

Public Attributes | List of all members
stdAc::state_t Struct Reference

Structure to hold a common A/C state. More...

`#include <IRsend.h>`

## Public Attributes

decode_type_t | protocol
int16_t | model
bool | power
stdAc::opmode_t | mode
float | degrees
bool | celsius
stdAc::fanspeed_t | fanspeed
stdAc::swingv_t | swingv
stdAc::swingh_t | swingh
bool | quiet
bool | turbo
bool | econo
bool | light
bool | filter
bool | clean
bool | beep
int16_t | sleep
int16_t | clock

## Detailed Description

Structure to hold a common A/C state.

## Member Data Documentation

## ◆ beep

bool stdAc::state_t::beep

## ◆ celsius

bool stdAc::state_t::celsius

## ◆ clean

bool stdAc::state_t::clean

## ◆ clock

int16_t stdAc::state_t::clock

## ◆ degrees

float stdAc::state_t::degrees

## ◆ econo

bool stdAc::state_t::econo

## ◆ fanspeed

stdAc::fanspeed_t stdAc::state_t::fanspeed

## ◆ filter

bool stdAc::state_t::filter

## ◆ light

bool stdAc::state_t::light

## ◆ mode

stdAc::opmode_t stdAc::state_t::mode

## ◆ model

int16_t stdAc::state_t::model

## ◆ power

bool stdAc::state_t::power

## ◆ protocol

decode_type_t stdAc::state_t::protocol

## ◆ quiet

bool stdAc::state_t::quiet

## ◆ sleep

int16_t stdAc::state_t::sleep

## ◆ swingh

stdAc::swingh_t stdAc::state_t::swingh

## ◆ swingv

stdAc::swingv_t stdAc::state_t::swingv

## ◆ turbo

bool stdAc::state_t::turbo

The documentation for this struct was generated from the following file:

- src/IRsend.h