IRremoteESP8266: Mitsubishi88Protocol Union Reference

IRremoteESP8266

Public Attributes | List of all members
Mitsubishi88Protocol Union Reference

Native representation of a Mitsubishi Heavy 88-bit A/C message. More...

`#include <ir_MitsubishiHeavy.h>`

## Public Attributes

uint8_t | raw [kMitsubishiHeavy88StateLength]
| State in code form. More...
struct {
uint8_t Sig [5]
uint8_t __pad0__:1
uint8_t SwingV5:1
uint8_t SwingH1:2
uint8_t __pad1__:1
uint8_t Clean:1
uint8_t SwingH2:2
uint8_t __pad2__:8
uint8_t __pad3__:3
uint8_t SwingV7:2
uint8_t Fan:3
uint8_t __pad4__:8
uint8_t Mode:3
uint8_t Power:1
uint8_t Temp:4
}; |

## Detailed Description

Native representation of a Mitsubishi Heavy 88-bit A/C message.

## Member Data Documentation

## ◆ @64

struct { ... }

## ◆ __pad0__

uint8_t Mitsubishi88Protocol::__pad0__

## ◆ __pad1__

uint8_t Mitsubishi88Protocol::__pad1__

## ◆ __pad2__

uint8_t Mitsubishi88Protocol::__pad2__

## ◆ __pad3__

uint8_t Mitsubishi88Protocol::__pad3__

## ◆ __pad4__

uint8_t Mitsubishi88Protocol::__pad4__

## ◆ Clean

uint8_t Mitsubishi88Protocol::Clean

## ◆ Fan

uint8_t Mitsubishi88Protocol::Fan

## ◆ Mode

uint8_t Mitsubishi88Protocol::Mode

## ◆ Power

uint8_t Mitsubishi88Protocol::Power

## ◆ raw

uint8_t Mitsubishi88Protocol::raw[kMitsubishiHeavy88StateLength]

State in code form.

## ◆ Sig

uint8_t Mitsubishi88Protocol::Sig[5]

## ◆ SwingH1

uint8_t Mitsubishi88Protocol::SwingH1

## ◆ SwingH2

uint8_t Mitsubishi88Protocol::SwingH2

## ◆ SwingV5

uint8_t Mitsubishi88Protocol::SwingV5

## ◆ SwingV7

uint8_t Mitsubishi88Protocol::SwingV7

## ◆ Temp

uint8_t Mitsubishi88Protocol::Temp

The documentation for this union was generated from the following file:

- src/ir_MitsubishiHeavy.h