IRremoteESP8266: TechnibelProtocol Union Reference

IRremoteESP8266

Public Attributes | List of all members
TechnibelProtocol Union Reference

Native representation of a Technibel A/C message. More...

`#include <ir_Technibel.h>`

## Public Attributes

uint64_t | raw
struct {
uint8_t Sum:8
uint8_t Footer:8
uint8_t TimerHours:5
uint8_t __pad0__:3
uint8_t Temp:7
uint8_t __pad1__:1
uint8_t Fan:3
uint8_t __pad2__:1
uint8_t Sleep:1
uint8_t Swing:1
uint8_t UseFah:1
uint8_t TimerEnable:1
uint8_t Mode:4
uint8_t FanChange:1
uint8_t TempChange:1
uint8_t TimerChange:1
uint8_t Power:1
uint8_t Header:8
}; |

## Detailed Description

Native representation of a Technibel A/C message.

## Member Data Documentation

## ◆ @80

struct { ... }

## ◆ __pad0__

uint8_t TechnibelProtocol::__pad0__

## ◆ __pad1__

uint8_t TechnibelProtocol::__pad1__

## ◆ __pad2__

uint8_t TechnibelProtocol::__pad2__

## ◆ Fan

uint8_t TechnibelProtocol::Fan

## ◆ FanChange

uint8_t TechnibelProtocol::FanChange

## ◆ Footer

uint8_t TechnibelProtocol::Footer

## ◆ Header

uint8_t TechnibelProtocol::Header

## ◆ Mode

uint8_t TechnibelProtocol::Mode

## ◆ Power

uint8_t TechnibelProtocol::Power

## ◆ raw

uint64_t TechnibelProtocol::raw

## ◆ Sleep

uint8_t TechnibelProtocol::Sleep

## ◆ Sum

uint8_t TechnibelProtocol::Sum

## ◆ Swing

uint8_t TechnibelProtocol::Swing

## ◆ Temp

uint8_t TechnibelProtocol::Temp

## ◆ TempChange

uint8_t TechnibelProtocol::TempChange

## ◆ TimerChange

uint8_t TechnibelProtocol::TimerChange

## ◆ TimerEnable

uint8_t TechnibelProtocol::TimerEnable

## ◆ TimerHours

uint8_t TechnibelProtocol::TimerHours

## ◆ UseFah

uint8_t TechnibelProtocol::UseFah

The documentation for this union was generated from the following file:

- src/ir_Technibel.h