IRremoteESP8266: Member List

IRremoteESP8266

IRAmcorAc Member List

This is the complete list of members for IRAmcorAc, including all inherited members.

_ | IRAmcorAc | private
_irsend | IRAmcorAc | private
begin() | IRAmcorAc |
calcChecksum(const uint8_t state[], const uint16_t length=kAmcorStateLength) | IRAmcorAc | static
calibrate(void) | IRAmcorAc | inline
checksum(void) | IRAmcorAc | private
convertFan(const stdAc::fanspeed_t speed) | IRAmcorAc | static
convertMode(const stdAc::opmode_t mode) | IRAmcorAc | static
getFan(void) const | IRAmcorAc |
getMax(void) const | IRAmcorAc |
getMode(void) const | IRAmcorAc |
getPower(void) const | IRAmcorAc |
getRaw(void) | IRAmcorAc |
getTemp(void) const | IRAmcorAc |
IRAmcorAc(const uint16_t pin, const bool inverted=false, const bool use_modulation=true) | IRAmcorAc | explicit
off(void) | IRAmcorAc |
on(void) | IRAmcorAc |
send(const uint16_t repeat=kAmcorDefaultRepeat) | IRAmcorAc |
setFan(const uint8_t speed) | IRAmcorAc |
setMax(const bool on) | IRAmcorAc |
setMode(const uint8_t mode) | IRAmcorAc |
setPower(const bool state) | IRAmcorAc |
setRaw(const uint8_t state[]) | IRAmcorAc |
setTemp(const uint8_t temp) | IRAmcorAc |
stateReset() | IRAmcorAc |
toCommon(void) const | IRAmcorAc |
toCommonFanSpeed(const uint8_t speed) | IRAmcorAc | static
toCommonMode(const uint8_t mode) | IRAmcorAc | static
toString(void) const | IRAmcorAc |
validChecksum(const uint8_t state[], const uint16_t length=kAmcorStateLength) | IRAmcorAc | static