IRremoteESP8266: Member List

IRremoteESP8266

IRSharpAc Member List

This is the complete list of members for IRSharpAc, including all inherited members.

_ | IRSharpAc | private
_fan | IRSharpAc | private
_getEconoToggle(void) const | IRSharpAc | private
_irsend | IRSharpAc | private
_mode | IRSharpAc | private
_model | IRSharpAc | private
_setEconoToggle(const bool on) | IRSharpAc | private
_temp | IRSharpAc | private
begin(void) | IRSharpAc |
calcChecksum(uint8_t state[], const uint16_t length=kSharpAcStateLength) | IRSharpAc | privatestatic
calibrate(void) | IRSharpAc | inline
checksum(void) | IRSharpAc | private
clearPowerSpecial(void) | IRSharpAc | private
convertFan(const stdAc::fanspeed_t speed, const sharp_ac_remote_model_t model=sharp_ac_remote_model_t::A907) | IRSharpAc | static
convertMode(const stdAc::opmode_t mode) | IRSharpAc | static
getClean(void) const | IRSharpAc |
getEconoToggle(void) const | IRSharpAc |
getFan(void) const | IRSharpAc |
getIon(void) const | IRSharpAc |
getLightToggle(void) const | IRSharpAc |
getMode(void) const | IRSharpAc |
getModel(const bool raw=false) const | IRSharpAc |
getPower(void) const | IRSharpAc |
getPowerSpecial(void) const | IRSharpAc | private
getRaw(void) | IRSharpAc |
getSpecial(void) const | IRSharpAc |
getSwingToggle(void) const | IRSharpAc |
getTemp(void) const | IRSharpAc |
getTimerEnabled(void) const | IRSharpAc |
getTimerTime(void) const | IRSharpAc |
getTimerType(void) const | IRSharpAc |
getTurbo(void) const | IRSharpAc |
IRSharpAc(const uint16_t pin, const bool inverted=false, const bool use_modulation=true) | IRSharpAc | explicit
isPowerSpecial(void) const | IRSharpAc |
off(void) | IRSharpAc |
on(void) | IRSharpAc |
send(const uint16_t repeat=kSharpAcDefaultRepeat) | IRSharpAc |
setClean(const bool on) | IRSharpAc |
setEconoToggle(const bool on) | IRSharpAc |
setFan(const uint8_t fan, const bool save=true) | IRSharpAc |
setIon(const bool on) | IRSharpAc |
setLightToggle(const bool on) | IRSharpAc |
setMode(const uint8_t mode, const bool save=true) | IRSharpAc |
setModel(const sharp_ac_remote_model_t model) | IRSharpAc |
setPower(const bool on, const bool prev_on=true) | IRSharpAc |
setPowerSpecial(const uint8_t value) | IRSharpAc | inlineprivate
setRaw(const uint8_t new_code[], const uint16_t length=kSharpAcStateLength) | IRSharpAc |
setSpecial(const uint8_t mode) | IRSharpAc |
setSwingToggle(const bool on) | IRSharpAc |
setTemp(const uint8_t temp, const bool save=true) | IRSharpAc |
setTimer(bool enable, bool timer_type, uint16_t mins) | IRSharpAc |
setTurbo(const bool on) | IRSharpAc |
stateReset(void) | IRSharpAc | private
toCommon(void) const | IRSharpAc |
toCommonFanSpeed(const uint8_t speed) const | IRSharpAc |
toCommonMode(const uint8_t mode) const | IRSharpAc |
toString(void) const | IRSharpAc |
validChecksum(uint8_t state[], const uint16_t length=kSharpAcStateLength) | IRSharpAc | static