IRremoteESP8266: Member List

IRremoteESP8266

IRArgoAC Member List

This is the complete list of members for IRArgoAC, including all inherited members.

_ | IRArgoAC | private
_irsend | IRArgoAC | private
begin(void) | IRArgoAC |
calcChecksum(const uint8_t state[], const uint16_t length=kArgoStateLength) | IRArgoAC | static
calibrate(void) | IRArgoAC | inline
checksum(void) | IRArgoAC | private
convertFan(const stdAc::fanspeed_t speed) | IRArgoAC | static
convertMode(const stdAc::opmode_t mode) | IRArgoAC | static
convertSwingV(const stdAc::swingv_t position) | IRArgoAC | static
cool_mode | IRArgoAC | private
flap_mode | IRArgoAC | private
getFan(void) const | IRArgoAC |
getFlap(void) const | IRArgoAC |
getiFeel(void) const | IRArgoAC |
getMax(void) const | IRArgoAC |
getMode(void) const | IRArgoAC |
getNight(void) const | IRArgoAC |
getPower(void) const | IRArgoAC |
getRaw(void) | IRArgoAC |
getRoomTemp(void) const | IRArgoAC |
getTemp(void) const | IRArgoAC |
heat_mode | IRArgoAC | private
IRArgoAC(const uint16_t pin, const bool inverted=false, const bool use_modulation=true) | IRArgoAC | explicit
off(void) | IRArgoAC |
on(void) | IRArgoAC |
send(const uint16_t repeat=kArgoDefaultRepeat) | IRArgoAC |
setFan(const uint8_t fan) | IRArgoAC |
setFlap(const uint8_t flap) | IRArgoAC |
setiFeel(const bool on) | IRArgoAC |
setMax(const bool on) | IRArgoAC |
setMode(const uint8_t mode) | IRArgoAC |
setNight(const bool on) | IRArgoAC |
setPower(const bool on) | IRArgoAC |
setRaw(const uint8_t state[]) | IRArgoAC |
setRoomTemp(const uint8_t degrees) | IRArgoAC |
setTemp(const uint8_t degrees) | IRArgoAC |
setTime(void) | IRArgoAC |
stateReset(void) | IRArgoAC | private
toCommon(void) const | IRArgoAC |
toCommonFanSpeed(const uint8_t speed) | IRArgoAC | static
toCommonMode(const uint8_t mode) | IRArgoAC | static
toString(void) const | IRArgoAC |
validChecksum(const uint8_t state[], const uint16_t length=kArgoStateLength) | IRArgoAC | static