IRremoteESP8266: Member List

IRremoteESP8266

IRFujitsuAC Member List

This is the complete list of members for IRFujitsuAC, including all inherited members.

_clean | IRFujitsuAC | private
_cmd | IRFujitsuAC | private
_fanSpeed | IRFujitsuAC | private
_filter | IRFujitsuAC | private
_irsend | IRFujitsuAC | private
_mode | IRFujitsuAC | private
_model | IRFujitsuAC | private
_offtimer | IRFujitsuAC | private
_ontimer | IRFujitsuAC | private
_outsideQuiet | IRFujitsuAC | private
_state_length | IRFujitsuAC | private
_state_length_short | IRFujitsuAC | private
_swingMode | IRFujitsuAC | private
_temp | IRFujitsuAC | private
_timertype | IRFujitsuAC | private
begin(void) | IRFujitsuAC |
buildFromState(const uint16_t length) | IRFujitsuAC | private
buildState(void) | IRFujitsuAC | private
calibrate(void) | IRFujitsuAC | inline
convertFan(stdAc::fanspeed_t speed) | IRFujitsuAC |
convertMode(const stdAc::opmode_t mode) | IRFujitsuAC |
getClean(const bool raw=false) | IRFujitsuAC |
getCmd(const bool raw=false) | IRFujitsuAC |
getFanSpeed(void) | IRFujitsuAC |
getFilter(const bool raw=false) | IRFujitsuAC |
getMode(void) | IRFujitsuAC |
getModel(void) | IRFujitsuAC |
getOffSleepTimer(const bool raw=false) | IRFujitsuAC |
getOnTimer(const bool raw=false) | IRFujitsuAC |
getOutsideQuiet(const bool raw=false) | IRFujitsuAC |
getPower(void) | IRFujitsuAC |
getRaw(void) | IRFujitsuAC |
getStateLength(void) | IRFujitsuAC |
getSwing(const bool raw=false) | IRFujitsuAC |
getTemp(void) | IRFujitsuAC |
getTimerType(const bool raw=false) | IRFujitsuAC |
IRFujitsuAC(const uint16_t pin, const fujitsu_ac_remote_model_t model=ARRAH2E, const bool inverted=false, const bool use_modulation=true) | IRFujitsuAC | explicit
off(void) | IRFujitsuAC |
on(void) | IRFujitsuAC |
remote_state | IRFujitsuAC | private
send(const uint16_t repeat=kFujitsuAcMinRepeat) | IRFujitsuAC |
setClean(const bool on) | IRFujitsuAC |
setCmd(const uint8_t cmd) | IRFujitsuAC |
setFanSpeed(const uint8_t fan) | IRFujitsuAC |
setFilter(const bool on) | IRFujitsuAC |
setMode(const uint8_t mode) | IRFujitsuAC |
setModel(const fujitsu_ac_remote_model_t model) | IRFujitsuAC |
setOffSleepTimer(const uint16_t nr_mins) | IRFujitsuAC | private
setOffTimer(const uint16_t nr_mins) | IRFujitsuAC |
setOnTimer(const uint16_t nr_mins) | IRFujitsuAC |
setOutsideQuiet(const bool on) | IRFujitsuAC |
setPower(const bool on) | IRFujitsuAC |
setRaw(const uint8_t newState[], const uint16_t length) | IRFujitsuAC |
setSleepTimer(const uint16_t nr_mins) | IRFujitsuAC |
setSwing(const uint8_t mode) | IRFujitsuAC |
setTemp(const uint8_t temp) | IRFujitsuAC |
setTimerType(const uint8_t timertype) | IRFujitsuAC |
stateReset(void) | IRFujitsuAC |
stepHoriz(void) | IRFujitsuAC |
stepVert(void) | IRFujitsuAC |
toCommon(void) | IRFujitsuAC |
toCommonFanSpeed(const uint8_t speed) | IRFujitsuAC | static
toCommonMode(const uint8_t mode) | IRFujitsuAC | static
toggleSwingHoriz(const bool update=true) | IRFujitsuAC |
toggleSwingVert(const bool update=true) | IRFujitsuAC |
toString(void) | IRFujitsuAC |
validChecksum(uint8_t *state, const uint16_t length) | IRFujitsuAC | static