IRremoteESP8266: Member List

IRremoteESP8266

IRMitsubishi136 Member List

This is the complete list of members for IRMitsubishi136, including all inherited members.

_ | IRMitsubishi136 | private
_irsend | IRMitsubishi136 | private
begin(void) | IRMitsubishi136 |
calibrate(void) | IRMitsubishi136 | inline
checksum(void) | IRMitsubishi136 | private
convertFan(const stdAc::fanspeed_t speed) | IRMitsubishi136 | static
convertMode(const stdAc::opmode_t mode) | IRMitsubishi136 | static
convertSwingV(const stdAc::swingv_t position) | IRMitsubishi136 | static
getFan(void) const | IRMitsubishi136 |
getMode(void) const | IRMitsubishi136 |
getPower(void) const | IRMitsubishi136 |
getQuiet(void) const | IRMitsubishi136 |
getRaw(void) | IRMitsubishi136 |
getSwingV(void) const | IRMitsubishi136 |
getTemp(void) const | IRMitsubishi136 |
IRMitsubishi136(const uint16_t pin, const bool inverted=false, const bool use_modulation=true) | IRMitsubishi136 | explicit
off(void) | IRMitsubishi136 |
on(void) | IRMitsubishi136 |
send(const uint16_t repeat=kMitsubishi136MinRepeat) | IRMitsubishi136 |
setFan(const uint8_t speed) | IRMitsubishi136 |
setMode(const uint8_t mode) | IRMitsubishi136 |
setPower(const bool on) | IRMitsubishi136 |
setQuiet(const bool on) | IRMitsubishi136 |
setRaw(const uint8_t *data) | IRMitsubishi136 |
setSwingV(const uint8_t position) | IRMitsubishi136 |
setTemp(const uint8_t degrees) | IRMitsubishi136 |
stateReset(void) | IRMitsubishi136 |
toCommon(void) const | IRMitsubishi136 |
toCommonFanSpeed(const uint8_t speed) | IRMitsubishi136 | static
toCommonMode(const uint8_t mode) | IRMitsubishi136 | static
toCommonSwingV(const uint8_t pos) | IRMitsubishi136 | static
toString(void) const | IRMitsubishi136 |
validChecksum(const uint8_t *data, const uint16_t len=kMitsubishi136StateLength) | IRMitsubishi136 | static