IRremoteESP8266: Member List

IRremoteESP8266

IRToshibaAC Member List

This is the complete list of members for IRToshibaAC, including all inherited members.

_ | IRToshibaAC | private
_backupState(void) | IRToshibaAC | private
_irsend | IRToshibaAC | private
_prev_mode | IRToshibaAC | private
_restoreState(void) | IRToshibaAC | private
_send_swing | IRToshibaAC | private
_swing_mode | IRToshibaAC | private
backup | IRToshibaAC | private
begin(void) | IRToshibaAC |
calcChecksum(const uint8_t state[], const uint16_t length=kToshibaACStateLength) | IRToshibaAC | privatestatic
calibrate(void) | IRToshibaAC | inline
checksum(const uint16_t length=kToshibaACStateLength) | IRToshibaAC | private
convertFan(const stdAc::fanspeed_t speed) | IRToshibaAC | static
convertMode(const stdAc::opmode_t mode) | IRToshibaAC | static
getEcono(void) const | IRToshibaAC |
getFan(void) const | IRToshibaAC |
getInternalStateLength(const uint8_t state[], const uint16_t size) | IRToshibaAC | static
getMode(const bool raw=false) const | IRToshibaAC |
getPower(void) const | IRToshibaAC |
getRaw(void) | IRToshibaAC |
getStateLength(void) const | IRToshibaAC |
getSwing(const bool raw=true) const | IRToshibaAC |
getTemp(void) const | IRToshibaAC |
getTurbo(void) const | IRToshibaAC |
IRToshibaAC(const uint16_t pin, const bool inverted=false, const bool use_modulation=true) | IRToshibaAC | explicit
off(void) | IRToshibaAC |
on(void) | IRToshibaAC |
send(const uint16_t repeat=kToshibaACMinRepeat) | IRToshibaAC |
setEcono(const bool on) | IRToshibaAC |
setFan(const uint8_t speed) | IRToshibaAC |
setMode(const uint8_t mode) | IRToshibaAC |
setPower(const bool on) | IRToshibaAC |
setRaw(const uint8_t newState[]) | IRToshibaAC |
setStateLength(const uint16_t size) | IRToshibaAC | private
setSwing(const uint8_t setting) | IRToshibaAC |
setTemp(const uint8_t degrees) | IRToshibaAC |
setTurbo(const bool on) | IRToshibaAC |
stateReset(void) | IRToshibaAC |
toCommon(void) const | IRToshibaAC |
toCommonFanSpeed(const uint8_t speed) | IRToshibaAC | static
toCommonMode(const uint8_t mode) | IRToshibaAC | static
toString(void) const | IRToshibaAC |
validChecksum(const uint8_t state[], const uint16_t length=kToshibaACStateLength) | IRToshibaAC | static