IRremoteESP8266: Member List

IRremoteESP8266

IRTranscoldAc Member List

This is the complete list of members for IRTranscoldAc, including all inherited members.

_ | IRTranscoldAc | private
_irsend | IRTranscoldAc | private
begin(void) | IRTranscoldAc |
calibrate(void) | IRTranscoldAc | inline
convertFan(const stdAc::fanspeed_t speed) | IRTranscoldAc | static
convertMode(const stdAc::opmode_t mode) | IRTranscoldAc | static
getFan(void) const | IRTranscoldAc |
getMode(void) const | IRTranscoldAc |
getPower(void) const | IRTranscoldAc |
getRaw(void) const | IRTranscoldAc |
getSwing(void) const | IRTranscoldAc |
getTemp(void) const | IRTranscoldAc |
handleSpecialState(const uint32_t data) | IRTranscoldAc | private
IRTranscoldAc(const uint16_t pin, const bool inverted=false, const bool use_modulation=true) | IRTranscoldAc | explicit
isSpecialState(void) const | IRTranscoldAc | private
off(void) | IRTranscoldAc |
on(void) | IRTranscoldAc |
send(const uint16_t repeat=kTranscoldDefaultRepeat) | IRTranscoldAc |
setFan(const uint8_t speed, const bool modecheck=true) | IRTranscoldAc |
setMode(const uint8_t mode) | IRTranscoldAc |
setPower(const bool state) | IRTranscoldAc |
setRaw(const uint32_t new_code) | IRTranscoldAc |
setSwing(void) | IRTranscoldAc |
setTemp(const uint8_t temp) | IRTranscoldAc |
special_state | IRTranscoldAc | private
stateReset(void) | IRTranscoldAc |
swingFlag | IRTranscoldAc | private
swingHFlag | IRTranscoldAc | private
swingVFlag | IRTranscoldAc | private
toCommon(const stdAc::state_t *prev=NULL) const | IRTranscoldAc |
toCommonFanSpeed(const uint8_t speed) | IRTranscoldAc | static
toCommonMode(const uint8_t mode) | IRTranscoldAc | static
toString(void) const | IRTranscoldAc |