IRremoteESP8266: Member List

IRremoteESP8266

IRPanasonicAc Member List

This is the complete list of members for IRPanasonicAc, including all inherited members.

_getTime(const uint8_t ptr[]) | IRPanasonicAc | privatestatic
_irsend | IRPanasonicAc | private
_setTime(uint8_t *const ptr, const uint16_t mins_since_midnight, const bool round_down) | IRPanasonicAc | privatestatic
_swingh | IRPanasonicAc | private
_temp | IRPanasonicAc | private
begin(void) | IRPanasonicAc |
calcChecksum(const uint8_t *state, const uint16_t length=kPanasonicAcStateLength) | IRPanasonicAc | static
calibrate(void) | IRPanasonicAc | inline
cancelOffTimer(void) | IRPanasonicAc |
cancelOnTimer(void) | IRPanasonicAc |
convertFan(const stdAc::fanspeed_t speed) | IRPanasonicAc | static
convertMode(const stdAc::opmode_t mode) | IRPanasonicAc | static
convertSwingH(const stdAc::swingh_t position) | IRPanasonicAc | static
convertSwingV(const stdAc::swingv_t position) | IRPanasonicAc | static
encodeTime(const uint8_t hours, const uint8_t mins) | IRPanasonicAc | static
fixChecksum(const uint16_t length=kPanasonicAcStateLength) | IRPanasonicAc | private
getClock(void) | IRPanasonicAc |
getFan(void) | IRPanasonicAc |
getIon(void) | IRPanasonicAc |
getMode(void) | IRPanasonicAc |
getModel(void) | IRPanasonicAc |
getOffTimer(void) | IRPanasonicAc |
getOnTimer(void) | IRPanasonicAc |
getPower(void) | IRPanasonicAc |
getPowerful(void) | IRPanasonicAc |
getQuiet(void) | IRPanasonicAc |
getRaw(void) | IRPanasonicAc |
getSwingHorizontal(void) | IRPanasonicAc |
getSwingVertical(void) | IRPanasonicAc |
getTemp(void) | IRPanasonicAc |
IRPanasonicAc(const uint16_t pin, const bool inverted=false, const bool use_modulation=true) | IRPanasonicAc | explicit
isOffTimerEnabled(void) | IRPanasonicAc |
isOnTimerEnabled(void) | IRPanasonicAc |
off(void) | IRPanasonicAc |
on(void) | IRPanasonicAc |
remote_state | IRPanasonicAc | private
send(const uint16_t repeat=kPanasonicAcDefaultRepeat) | IRPanasonicAc |
setClock(const uint16_t mins_since_midnight) | IRPanasonicAc |
setFan(const uint8_t fan) | IRPanasonicAc |
setIon(const bool on) | IRPanasonicAc |
setMode(const uint8_t mode) | IRPanasonicAc |
setModel(const panasonic_ac_remote_model_t model) | IRPanasonicAc |
setOffTimer(const uint16_t mins_since_midnight, const bool enable=true) | IRPanasonicAc |
setOnTimer(const uint16_t mins_since_midnight, const bool enable=true) | IRPanasonicAc |
setPower(const bool on) | IRPanasonicAc |
setPowerful(const bool on) | IRPanasonicAc |
setQuiet(const bool on) | IRPanasonicAc |
setRaw(const uint8_t state[]) | IRPanasonicAc |
setSwingHorizontal(const uint8_t direction) | IRPanasonicAc |
setSwingVertical(const uint8_t elevation) | IRPanasonicAc |
setTemp(const uint8_t temp, const bool remember=true) | IRPanasonicAc |
stateReset(void) | IRPanasonicAc |
toCommon(void) | IRPanasonicAc |
toCommonFanSpeed(const uint8_t speed) | IRPanasonicAc | static
toCommonMode(const uint8_t mode) | IRPanasonicAc | static
toCommonSwingH(const uint8_t pos) | IRPanasonicAc | static
toCommonSwingV(const uint8_t pos) | IRPanasonicAc | static
toString(void) | IRPanasonicAc |
validChecksum(const uint8_t *state, const uint16_t length=kPanasonicAcStateLength) | IRPanasonicAc | static