IRremoteESP8266: IRTcl112Ac Class Reference

IRremoteESP8266

Public Member Functions | Static Public Member Functions | Private Member Functions | Private Attributes | List of all members
IRTcl112Ac Class Reference

Class for handling detailed TCL A/C messages. More...

`#include <ir_Tcl.h>`

Collaboration diagram for IRTcl112Ac:
[legend]

## Public Member Functions

| IRTcl112Ac (const uint16_t pin, const bool inverted=false, const bool use_modulation=true)
| Class constructor. More...
void | send (const uint16_t repeat=kTcl112AcDefaultRepeat)
| Send the current internal state as an IR message. More...
int8_t | calibrate (void)
| Run the calibration to calculate uSec timing offsets for this platform. More...
void | begin (void)
| Set up hardware to be able to send a message. More...
void | stateReset (void)
| Reset the internal state of the emulation. (On, Cool, 24C) More...
uint8_t * | getRaw (void)
| Get a PTR to the internal state/code for this protocol. More...
void | setRaw (const uint8_t new_code[], const uint16_t length=kTcl112AcStateLength)
| Set the internal state from a valid code for this protocol. More...
void | on (void)
| Set the requested power state of the A/C to on. More...
void | off (void)
| Set the requested power state of the A/C to off. More...
void | setPower (const bool on)
| Change the power setting. More...
bool | getPower (void) const
| Get the value of the current power setting. More...
void | setTemp (const float celsius)
| Set the temperature. More...
float | getTemp (void) const
| Get the current temperature setting. More...
void | setMode (const uint8_t mode)
| Set the operating mode of the A/C. More...
uint8_t | getMode (void) const
| Get the operating mode setting of the A/C. More...
void | setFan (const uint8_t speed)
| Set the speed of the fan. More...
uint8_t | getFan (void) const
| Get the current fan speed setting. More...
void | setEcono (const bool on)
| Set the economy setting of the A/C. More...
bool | getEcono (void) const
| Get the economy setting of the A/C. More...
void | setHealth (const bool on)
| Set the Health (Filter) setting of the A/C. More...
bool | getHealth (void) const
| Get the Health (Filter) setting of the A/C. More...
void | setLight (const bool on)
| Set the Light (LED/Display) setting of the A/C. More...
bool | getLight (void) const
| Get the Light (LED/Display) setting of the A/C. More...
void | setSwingHorizontal (const bool on)
| Set the horizontal swing setting of the A/C. More...
bool | getSwingHorizontal (void) const
| Get the horizontal swing setting of the A/C. More...
void | setSwingVertical (const bool on)
| Set the vertical swing setting of the A/C. More...
bool | getSwingVertical (void) const
| Get the vertical swing setting of the A/C. More...
void | setTurbo (const bool on)
| Set the Turbo setting of the A/C. More...
bool | getTurbo (void) const
| Get the Turbo setting of the A/C. More...
stdAc::state_t | toCommon (void) const
| Convert the current internal state into its stdAc::state_t equivalent. More...
String | toString (void) const
| Convert the current internal state into a human readable string. More...

## Static Public Member Functions

static uint8_t | calcChecksum (uint8_t state[], const uint16_t length=kTcl112AcStateLength)
| Calculate the checksum for a given state. More...
static bool | validChecksum (uint8_t state[], const uint16_t length=kTcl112AcStateLength)
| Verify the checksum is valid for a given state. More...
static uint8_t | convertMode (const stdAc::opmode_t mode)
| Convert a stdAc::opmode_t enum into its native mode. More...
static uint8_t | convertFan (const stdAc::fanspeed_t speed)
| Convert a stdAc::fanspeed_t enum into it's native speed. More...
static stdAc::opmode_t | toCommonMode (const uint8_t mode)
| Convert a native mode into its stdAc equivalent. More...
static stdAc::fanspeed_t | toCommonFanSpeed (const uint8_t speed)
| Convert a native fan speed into its stdAc equivalent. More...

## Private Member Functions

void | checksum (const uint16_t length=kTcl112AcStateLength)
| Calculate & set the checksum for the current internal state of the remote. More...

## Private Attributes

IRsend | _irsend
| Instance of the IR send class. More...
Tcl112Protocol | _

## Detailed Description

Class for handling detailed TCL A/C messages.

## Constructor & Destructor Documentation

## ◆ IRTcl112Ac()

IRTcl112Ac::IRTcl112Ac | ( | const uint16_t | pin,
|  | const bool | inverted = `false`,
|  | const bool | use_modulation = `true`
| ) |  |

explicit

Class constructor.

Parameters

  [in] | pin | GPIO to be used when sending.
  [in] | inverted | Is the output signal to be inverted?
  [in] | use_modulation | Is frequency modulation to be used?

## Member Function Documentation

## ◆ begin()

void IRTcl112Ac::begin | ( | void |  | ) |

Set up hardware to be able to send a message.

## ◆ calcChecksum()

uint8_t IRTcl112Ac::calcChecksum | ( | uint8_t | state[],
|  | const uint16_t | length = `kTcl112AcStateLength`
| ) |  |

static

Calculate the checksum for a given state.

Parameters

  [in] | state | The array to calc the checksum of.
  [in] | length | The length/size of the array.

Returns
  The calculated checksum value.

## ◆ calibrate()

int8_t IRTcl112Ac::calibrate | ( | void |  | ) |

inline

Run the calibration to calculate uSec timing offsets for this platform.

Returns
  The uSec timing offset needed per modulation of the IR Led.

Note
  This will produce a 65ms IR signal pulse at 38kHz. Only ever needs to be run once per object instantiation, if at all.

## ◆ checksum()

void IRTcl112Ac::checksum | ( | const uint16_t | length = `kTcl112AcStateLength` | ) |

private

Calculate & set the checksum for the current internal state of the remote.

Parameters

  [in] | length | The length/size of the internal array to checksum.

## ◆ convertFan()

uint8_t IRTcl112Ac::convertFan | ( | const stdAc::fanspeed_t | speed | ) |

static

Convert a stdAc::fanspeed_t enum into it's native speed.

Parameters

  [in] | speed | The enum to be converted.

Returns
  The native equivalent of the enum.

## ◆ convertMode()

uint8_t IRTcl112Ac::convertMode | ( | const stdAc::opmode_t | mode | ) |

static

Convert a stdAc::opmode_t enum into its native mode.

Parameters

  [in] | mode | The enum to be converted.

Returns
  The native equivalent of the enum.

## ◆ getEcono()

bool IRTcl112Ac::getEcono | ( | void |  | ) | const

Get the economy setting of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## ◆ getFan()

uint8_t IRTcl112Ac::getFan | ( | void |  | ) | const

Get the current fan speed setting.

Returns
  The current fan speed/mode.

## ◆ getHealth()

bool IRTcl112Ac::getHealth | ( | void |  | ) | const

Get the Health (Filter) setting of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## ◆ getLight()

bool IRTcl112Ac::getLight | ( | void |  | ) | const

Get the Light (LED/Display) setting of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## ◆ getMode()

uint8_t IRTcl112Ac::getMode | ( | void |  | ) | const

Get the operating mode setting of the A/C.

Returns
  The current operating mode setting.

## ◆ getPower()

bool IRTcl112Ac::getPower | ( | void |  | ) | const

Get the value of the current power setting.

Returns
  true, the setting is on. false, the setting is off.

## ◆ getRaw()

uint8_t * IRTcl112Ac::getRaw | ( | void |  | ) |

Get a PTR to the internal state/code for this protocol.

Returns
  PTR to a code for this protocol based on the current internal state.

## ◆ getSwingHorizontal()

bool IRTcl112Ac::getSwingHorizontal | ( | void |  | ) | const

Get the horizontal swing setting of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## ◆ getSwingVertical()

bool IRTcl112Ac::getSwingVertical | ( | void |  | ) | const

Get the vertical swing setting of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## ◆ getTemp()

float IRTcl112Ac::getTemp | ( | void |  | ) | const

Get the current temperature setting.

Returns
  The current setting for temp. in degrees celsius.

Note
  The temperature resolution is 0.5 of a degree.

## ◆ getTurbo()

bool IRTcl112Ac::getTurbo | ( | void |  | ) | const

Get the Turbo setting of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## ◆ off()

void IRTcl112Ac::off | ( | void |  | ) |

Set the requested power state of the A/C to off.

## ◆ on()

void IRTcl112Ac::on | ( | void |  | ) |

Set the requested power state of the A/C to on.

## ◆ send()

void IRTcl112Ac::send | ( | const uint16_t | repeat = `kTcl112AcDefaultRepeat` | ) |

Send the current internal state as an IR message.

Parameters

  [in] | repeat | Nr. of times the message will be repeated.

## ◆ setEcono()

void IRTcl112Ac::setEcono | ( | const bool | on | ) |

Set the economy setting of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## ◆ setFan()

void IRTcl112Ac::setFan | ( | const uint8_t | speed | ) |

Set the speed of the fan.

Parameters

  [in] | speed | The desired setting.

Note
  Unknown speeds will default to Auto.

## ◆ setHealth()

void IRTcl112Ac::setHealth | ( | const bool | on | ) |

Set the Health (Filter) setting of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## ◆ setLight()

void IRTcl112Ac::setLight | ( | const bool | on | ) |

Set the Light (LED/Display) setting of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## ◆ setMode()

void IRTcl112Ac::setMode | ( | const uint8_t | mode | ) |

Set the operating mode of the A/C.

Parameters

  [in] | mode | The desired operating mode.

Note
  Fan/Ventilation mode sets the fan speed to high. Unknown values default to Auto.

## ◆ setPower()

void IRTcl112Ac::setPower | ( | const bool | on | ) |

Change the power setting.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## ◆ setRaw()

void IRTcl112Ac::setRaw | ( | const uint8_t | new_code[],
|  | const uint16_t | length = `kTcl112AcStateLength`
| ) |  |

Set the internal state from a valid code for this protocol.

Parameters

  [in] | new_code | A valid code for this protocol.
  [in] | length | The length/size of the new_code array.

## ◆ setSwingHorizontal()

void IRTcl112Ac::setSwingHorizontal | ( | const bool | on | ) |

Set the horizontal swing setting of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## ◆ setSwingVertical()

void IRTcl112Ac::setSwingVertical | ( | const bool | on | ) |

Set the vertical swing setting of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## ◆ setTemp()

void IRTcl112Ac::setTemp | ( | const float | celsius | ) |

Set the temperature.

Parameters

  [in] | celsius | The temperature in degrees celsius.

Note
  The temperature resolution is 0.5 of a degree.

## ◆ setTurbo()

void IRTcl112Ac::setTurbo | ( | const bool | on | ) |

Set the Turbo setting of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## ◆ stateReset()

void IRTcl112Ac::stateReset | ( | void |  | ) |

Reset the internal state of the emulation. (On, Cool, 24C)

## ◆ toCommon()

stdAc::state_t IRTcl112Ac::toCommon | ( | void |  | ) | const

Convert the current internal state into its stdAc::state_t equivalent.

Returns
  The stdAc equivalent of the native settings.

## ◆ toCommonFanSpeed()

stdAc::fanspeed_t IRTcl112Ac::toCommonFanSpeed | ( | const uint8_t | spd | ) |

static

Convert a native fan speed into its stdAc equivalent.

Parameters

  [in] | spd | The native setting to be converted.

Returns
  The stdAc equivalent of the native setting.

## ◆ toCommonMode()

stdAc::opmode_t IRTcl112Ac::toCommonMode | ( | const uint8_t | mode | ) |

static

Convert a native mode into its stdAc equivalent.

Parameters

  [in] | mode | The native setting to be converted.

Returns
  The stdAc equivalent of the native setting.

## ◆ toString()

String IRTcl112Ac::toString | ( | void |  | ) | const

Convert the current internal state into a human readable string.

Returns
  A human readable string.

## ◆ validChecksum()

bool IRTcl112Ac::validChecksum | ( | uint8_t | state[],
|  | const uint16_t | length = `kTcl112AcStateLength`
| ) |  |

static

Verify the checksum is valid for a given state.

Parameters

  [in] | state | The array to verify the checksum of.
  [in] | length | The length/size of the array.

Returns
  true, if the state has a valid checksum. Otherwise, false.

## Member Data Documentation

## ◆ _

Tcl112Protocol IRTcl112Ac::_

private

## ◆ _irsend

IRsend IRTcl112Ac::_irsend

private

Instance of the IR send class.

The documentation for this class was generated from the following files:

- src/ir_Tcl.h
- src/ir_Tcl.cpp