IRremoteESP8266: Daikin160Protocol Union Reference

IRremoteESP8266

Public Attributes | List of all members
Daikin160Protocol Union Reference

Native representation of a Daikin160 A/C message. More...

`#include <ir_Daikin.h>`

## Public Attributes

uint8_t | raw [kDaikin160StateLength]
| The state of the IR remote. More...
struct {
uint8_t pad0 [6]
uint8_t Sum1:8
uint8_t pad1 [5]
uint8_t Power:1
uint8_t __pad0__:3
uint8_t Mode:3
uint8_t __pad1__:1
uint8_t __pad2__:4
uint8_t SwingV:4
uint8_t pad2 [2]
uint8_t __pad3__:1
uint8_t Temp:6
uint8_t __pad4__:1
uint8_t Fan:4
uint8_t __pad5__:4
uint8_t __pad6__:8
uint8_t Sum2:8
}; |

## Detailed Description

Native representation of a Daikin160 A/C message.

## Member Data Documentation

## ◆ @21

struct { ... }

## ◆ __pad0__

uint8_t Daikin160Protocol::__pad0__

## ◆ __pad1__

uint8_t Daikin160Protocol::__pad1__

## ◆ __pad2__

uint8_t Daikin160Protocol::__pad2__

## ◆ __pad3__

uint8_t Daikin160Protocol::__pad3__

## ◆ __pad4__

uint8_t Daikin160Protocol::__pad4__

## ◆ __pad5__

uint8_t Daikin160Protocol::__pad5__

## ◆ __pad6__

uint8_t Daikin160Protocol::__pad6__

## ◆ Fan

uint8_t Daikin160Protocol::Fan

## ◆ Mode

uint8_t Daikin160Protocol::Mode

## ◆ pad0

uint8_t Daikin160Protocol::pad0[6]

## ◆ pad1

uint8_t Daikin160Protocol::pad1[5]

## ◆ pad2

uint8_t Daikin160Protocol::pad2[2]

## ◆ Power

uint8_t Daikin160Protocol::Power

## ◆ raw

uint8_t Daikin160Protocol::raw[kDaikin160StateLength]

The state of the IR remote.

## ◆ Sum1

uint8_t Daikin160Protocol::Sum1

## ◆ Sum2

uint8_t Daikin160Protocol::Sum2

## ◆ SwingV

uint8_t Daikin160Protocol::SwingV

## ◆ Temp

uint8_t Daikin160Protocol::Temp

The documentation for this union was generated from the following file:

- src/ir_Daikin.h