IRremoteESP8266: GoodweatherProtocol Union Reference

IRremoteESP8266

Public Attributes | List of all members
GoodweatherProtocol Union Reference

Native representation of a Goodweather A/C message. More...

`#include <ir_Goodweather.h>`

## Public Attributes

uint64_t | raw
| The state of the IR remote in IR code form. More...
struct {
uint8_t __pad0__:8
uint8_t Light:1
uint8_t __pad1__:2
uint8_t Turbo:1
uint8_t __pad2__:0
uint8_t Command:4
uint8_t __pad3__:0
uint8_t Sleep:1
uint8_t Power:1
uint8_t Swing:2
uint8_t AirFlow:1
uint8_t Fan:2
uint8_t __pad4__:0
uint8_t Temp:4
uint8_t __pad5__:1
uint8_t Mode:3
uint8_t __pad6__:0
}; |

## Detailed Description

Native representation of a Goodweather A/C message.

## Member Data Documentation

## ◆ @35

struct { ... }

## ◆ __pad0__

uint8_t GoodweatherProtocol::__pad0__

## ◆ __pad1__

uint8_t GoodweatherProtocol::__pad1__

## ◆ __pad2__

uint8_t GoodweatherProtocol::__pad2__

## ◆ __pad3__

uint8_t GoodweatherProtocol::__pad3__

## ◆ __pad4__

uint8_t GoodweatherProtocol::__pad4__

## ◆ __pad5__

uint8_t GoodweatherProtocol::__pad5__

## ◆ __pad6__

uint8_t GoodweatherProtocol::__pad6__

## ◆ AirFlow

uint8_t GoodweatherProtocol::AirFlow

## ◆ Command

uint8_t GoodweatherProtocol::Command

## ◆ Fan

uint8_t GoodweatherProtocol::Fan

## ◆ Light

uint8_t GoodweatherProtocol::Light

## ◆ Mode

uint8_t GoodweatherProtocol::Mode

## ◆ Power

uint8_t GoodweatherProtocol::Power

## ◆ raw

uint64_t GoodweatherProtocol::raw

The state of the IR remote in IR code form.

## ◆ Sleep

uint8_t GoodweatherProtocol::Sleep

## ◆ Swing

uint8_t GoodweatherProtocol::Swing

## ◆ Temp

uint8_t GoodweatherProtocol::Temp

## ◆ Turbo

uint8_t GoodweatherProtocol::Turbo

The documentation for this union was generated from the following file:

- src/ir_Goodweather.h