IRremoteESP8266: LGProtocol Union Reference

IRremoteESP8266

Public Attributes | List of all members
LGProtocol Union Reference

Native representation of a LG A/C message. More...

`#include <ir_LG.h>`

## Public Attributes

uint32_t | raw
| The state of the IR remote in IR code form. More...
struct {
uint32_t Sum:4
uint32_t Fan:3
uint32_t __pad0__:1
uint32_t Temp:4
uint32_t Mode:3
uint32_t __pad1__:3
uint32_t Power:2
uint32_t Sign:8
}; |

## Detailed Description

Native representation of a LG A/C message.

## Member Data Documentation

## ◆ @51

struct { ... }

## ◆ __pad0__

uint32_t LGProtocol::__pad0__

## ◆ __pad1__

uint32_t LGProtocol::__pad1__

## ◆ Fan

uint32_t LGProtocol::Fan

## ◆ Mode

uint32_t LGProtocol::Mode

## ◆ Power

uint32_t LGProtocol::Power

## ◆ raw

uint32_t LGProtocol::raw

The state of the IR remote in IR code form.

## ◆ Sign

uint32_t LGProtocol::Sign

## ◆ Sum

uint32_t LGProtocol::Sum

## ◆ Temp

uint32_t LGProtocol::Temp

The documentation for this union was generated from the following file:

- src/ir_LG.h